**How to upgrade firmware from 2.0.0.8 to 2.0.0.23 on ECS5510-48S**

**Topology:**

****

**Version:**

****

1. Set switch IP address.



1. Ping 192.168.2.1/24(TFTP server).

****

1. Copy firmware (lion\_edg-20032.ros) from TFTP server to switch.



1. Reload the switch and then check the version.



1. Finish

